| Code | Function | Status | Comments |
| --- | --- | --- | --- |
| 11000 | Read attic temperature | OK |  |
| 11100 | Set attic temperature | OK |  |
| 12000 | Read room temperature | OK |  |
| 12200 | Set room temperature | OK |  |
| 13000 | Read outdoor Temperature | OK |  |
| 14000 | Read power consumption | OK |  |
| 15000 | ~~Read fire alarm status~~ | N/A | Removed / Unnecessary |
| 16000 | Read burglar alarm | OK |  |
| 17000 | ~~Read water leakage~~ | N/A | Removed / Unnecessary |
| 17000 | Set burglar alarm | OK | Replaces the old 17000 |
| 18000 | Read stove status | OK |  |
| 19000 | Read window status | OK |  |
| 21000 | Read power outage | N/A | Removed / Unnecessary |
| 22000 | Read attic fan status | OK |  |
| 23000 | Set attic fan | OK |  |
| 25000 | Read indoor light status | OK |  |
| 26000 | Set indoor light on/off | OK |  |
| 27000 | Read outdoor light status | OK |  |
| 28000 | Set outdoor light on/off | OK |  |
| 34000 | Water leakage detected | OK |  |
| 35000 | Fire detected | OK |  |
| 36000 | Burglar detected | OK |  |